Mechanical Solutions

# Water Jet Cold Cutting Technique

Abrasive UHP water jet cutting at 40,000–50,000 PSI for precise metal cutting without creating a heat affected zone.

## Service overview

This service page is based on the official ROKN AL-TAQA company profile and organized into a website-friendly format.

- Cuts carbon steel, stainless steel, alloy steel, and thick-wall materials with accuracy.
- No heat, no sparks, and no ignition risk in hazardous areas (Zone I & II).
- Produces clean cutting with no heat impact on base metal.
- Minimizes downtime and is compatible with hydrocarbon environments.
- Useful for removing nozzles, cutting flanges, opening manways, replacing pipeline sections, and dismantling steel structures.
- Supported by straight cutting, circular cutting, bevel cutting, flange removal, nozzle cutting, and profile cutting heads.
- Profile cold cutting head can remotely open manholes in tanks.
- Straight cutting can also be performed remotely on tanks.

Request this service
All Service Pages

- Ultra High-Pressure Water Jet Pump→
- Cleaning by Ultra High-Pressure Water Jet Pump→
- Heat Exchanger Cleaning→
- Cooler Cleaning→
- Well Cleaning→
- Towers Cleaning→
- Tank Water Jet Blasting→
- Water Jet Cold Cutting Technique→
- Advanced NDT Inspection→
- Phased Array Ultrasonic Testing (PAUT)→
- Long-Range Ultrasonic Testing (LRUT)→
- Automatic Ultrasonic Testing (AUT)→
- Manual Ultrasonic Testing (MUT)→
- Welding Projects→
- Pigging→
- Hydrostatic Test→
- Flange Managements→
- Zero Flare Gases to Electricity→
- Chemical Cleaning→
- Supplying the Services Sector→

Integrated Capability

## Need this service inside a larger industrial package?

ROKN AL-TAQA positions this activity as part of a broader integrated services model across cleaning, inspection, fabrication, testing, and pipeline support.

Back to all services